1987 Nissan-Datsun 300ZX V6-2960cc 3.0L SOHC MFI (VG30E)
Top - Vehicle 
 Engine 
.  Technical Service Bulletins 
. .  All Technical Service Bulletins 
. . .  VG30 Engine Modifications
 
VG30 Engine Modifications
Models         All Models with VG30
Section        Engine Mechanical
Classification EM87-010
Bulletin No.   TS87-191
Date           December 28, 1987
VG30 ENGINE MODIFICATIONS
APPLIED MODELS: All vehicles with VG30 Engine
 
Beginning with April, 1987 production, several major components of the VG30 engine have been changed to decrease noise levels and improve power output.

The MODIFIED AND NON-MODIFIED engines can be identified by the engine serial number as follows:

                                 MODIFIED                  NON-MODIFIED
                                                           (XXXXXX A)
                                (XXXXXX W)                       OR
                                                            (XXXXXX B)

The major engine components that have been changed to create the "W" engine are shown below, and on the following pages. In addition, a summary of changes is provided for each component.
CYLINDER BLOCK 
 
  Six new water galleries were added at the exhaust side of the cylinders.NOTE: The "W" engine bare block will NOT be stamped with a "W". Check for additional water galleries to identify a modified bare block.
 In addition, the oil pan bolt holes have been altered in the modified cylinder block. The holes have been chamfered to allow usage of a liquid oil pan gasket. These chamfered bolt holes are also helpful in identifying the modified bare block.
PISTON & PISTON PINS 
 The piston and pin have been changed to a full-floating type, with two snap rings to locate the piston pin. Also, piston pin outer diameter has been decreased.
The modified piston can be identified by a "W" mark on the piston skirt (As shown).

NOTE: A "W" piston requires a modified connecting rod, wrist pin, and piston rings. 
CONNECTING ROD 
 
  The modified connecting rod has been increased in weight, along with an increase in small end internal bore. It can be identified by a "W" stamped in the side of the rod shaft as shown in illustration.

NOTE: A "W" connecting rod requires a "W" piston, new style wrist pin, and modified crankshaft. 
CRANKSHAFT, PULLEY, BOLT & WASHER 

The crankshaft front tip was lengthened by 18.7 mm (0.736) in. See illustration (*1).

The crankshaft pulley width was increased by 13.6 mm (0.535 in.) as shown (*2).

The pulley bolt was changed from M12 to M14, and the washer inner and outer diameters were increased. (See illustration.)
CYLINDER HEAD 

Three new water galleries were added to each cylinder head (at the exhaust side). These match the new galleries in the block.
CYLINDER HEAD GASKET 

Three new holes were added to the gasket on the exhaust side, and the six holes in the intake side of the gasket were decreased in size.
CYLINDER HEAD GASKET IDENTIFICATION 

The tab shape can be used to identify the modified gasket from the non-modified gasket. (See illustration.)
 
  COMPONENT INTERCHANGEABILITY INFORMATION

In certain combinations, some MODIFIED engine components can be installed on NON-MODIFIED VG30 ENGINES (production prior to April, 1987) as shown in the following chart. However, NON-MODIFIED ENGINE COMPONENTS CANNOT BE INSTALLED ON MODIFIED VG30 ENGINES (production starting April, 1987).

Use the chart below to determine proper component combinations.(1) Refer to Parts Microfiche for complete application information.
 
(2) Modified short engine can be used in place of non-modified short engine in conjunction with the cylinder head/head gasket combinations shown as acceptable in chart on page 4/6. Also, the crank pulley must be changed as indicated below:
Truck, Pathfinder, 200SX, Maxima, and 300ZX (except 300ZX prior to 9/86 production), must use the modified crankshaft pulley, bolt and washer shown in the chart on page 6/6.
300ZX Non-Turbo prior to 9/86 production requires crankshaft pulley (P/N 12303-12G01, bolt (P/N 12309-16V00) and washer (P/N 12308-77A00). 300ZX Turbo prior to 9/86 production requires crankshaft pulley (P/N 12303 5320), spacer (P/N 12308-V5321), bolt (P/N 12309-16V00) and washer (P/N 12308-77A00).

 (3) Modified parts can be used in place of non-modified parts in combinations shown as acceptable in chart on page 4/6.